
**** 02/20/12 17:05:29 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_8\chap8_ex8-17-pspicefiles\schematic1\bias.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "bias.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
* From [PSPICE NETLIST] section of C:\OrCAD\OrCAD_10.5\tools\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.AC DEC 101 10 100meg
.PROBE V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\SCHEMATIC1.net" 



**** INCLUDING SCHEMATIC1.net ****
* source CHAP8_EX8-17
C_C1         N19467 VOUT  10  
C_C2         N19699 N19471  10  
V_V1         N19513 0 20
V_V2         N19661 0 DC 0Vdc AC 1Vac 
R_R1         N19471 N19513  150k  
R_R2         0 N19471  16k  
R_Rsi         N19661 N19699  1k  
R_RL         0 VOUT  10k  
M_M1         N19467 N19471 0 0 M2N6660
R_RD         N19467 N19513  10k  

**** RESUMING bias.cir ****
.END

**** 02/20/12 17:05:29 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_8\chap8_ex8-17-pspicefiles\schematic1\bias.sim ] 


 ****     MOSFET MODEL PARAMETERS


******************************************************************************




               M2N6660         
               NMOS            
       LEVEL    3            
           L    2.000000E-06 
           W     .32         
         VTO    1.8          
          KP    1.047000E-06 
       GAMMA    0            
         PHI     .6          
      LAMBDA    0            
          RD     .4672       
          RS     .02         
          RG  209.5          
          RB    1.000000E-03 
         RDS    6.000000E+06 
          IS   10.000000E-15 
          JS    0            
          PB     .8          
        PBSW     .8          
         CBD  118.000000E-12 
          CJ    0            
        CJSW    0            
        CGSO    1.885000E-12 
        CGDO    7.564000E-12 
        CGBO    0            
         TOX    2.000000E-06 
          XJ    0            
       UCRIT   10.000000E+03 
       DELTA    0            
         ETA    0            
      DIOMOD    1            
         VFB    0            
        LETA    0            
        WETA    0            
          U0    0            
        TEMP    0            
         VDD    0            
       XPART    0            


**** 02/20/12 17:05:29 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_8\chap8_ex8-17-pspicefiles\schematic1\bias.sim ] 


 ****     SMALL SIGNAL BIAS SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


( VOUT)    0.0000  (N19467)    6.3340 (N19471)    1.9277 (N19513)   20.0000     

(N19661)    0.0000 (N19699)    0.0000 




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_V1        -1.487E-03
    V_V2         0.000E+00

    TOTAL POWER DISSIPATION   2.97E-02  WATTS



          JOB CONCLUDED

**** 02/20/12 17:05:29 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_8\chap8_ex8-17-pspicefiles\schematic1\bias.sim ] 


 ****     JOB STATISTICS SUMMARY


******************************************************************************



  Total job time (using Solver 1)   =         .06
