
**** 02/17/12 14:26:40 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_8\chap8_ex8-9-pspicefiles\schematic1\bias.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "bias.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
.LIB "../../../chap8_ex8-9-pspicefiles/chap8_ex8-9.lib" 
* From [PSPICE NETLIST] section of C:\OrCAD\OrCAD_10.5\tools\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.AC DEC 101 1 100k
.PROBE V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\SCHEMATIC1.net" 



**** INCLUDING SCHEMATIC1.net ****
* source CHAP8_EX8-9
C_Cc         N06872 VOUT  1uF  
R_RD         N06872 VCC  14k  
R_R2         0 N06105  33k  
V_V4         0 VEE 10v
R_R1         N06105 VCC  160k  
C_Cc1         N06137 N06105  10  
V_V3         N06137 0 DC 0Vdc AC 1Vac 
R_RS         0 N06291  0.5k  
V_V2         VCC 0 10v
R_RL         0 VOUT  14k  
M_M1         N06872 N06105 N06291 0 Mbreakn  
+ L=3u  
+ W=75u         

**** RESUMING bias.cir ****
.END

**** 02/17/12 14:26:40 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_8\chap8_ex8-9-pspicefiles\schematic1\bias.sim ] 


 ****     MOSFET MODEL PARAMETERS


******************************************************************************




               Mbreakn         
               NMOS            
       LEVEL    3            
           L    2.000000E-06 
           W     .75         
         VTO    3            
          KP    1.035943E-06 
       GAMMA    0            
         PHI     .6          
      LAMBDA    0            
          RD     .01         
          RS     .01         
          RG    5            
          RB    1.000000E-03 
         RDS    1.000000E+06 
          IS   10.000000E-15 
          JS    0            
          PB     .8          
        PBSW     .8          
         CBD    1.000000E-09 
          CJ    0            
        CJSW    0            
        CGSO   40.000000E-12 
        CGDO   10.000000E-12 
        CGBO    0            
         TOX    2.000000E-06 
          XJ    0            
       UCRIT   10.000000E+03 
       KAPPA    1.000000E-12 
      DIOMOD    1            
         VFB    0            
        LETA    0            
        WETA    0            
          U0    0            
        TEMP    0            
         VDD    0            
       XPART    0            


**** 02/17/12 14:26:40 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_8\chap8_ex8-9-pspicefiles\schematic1\bias.sim ] 


 ****     SMALL SIGNAL BIAS SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(  VCC)   10.0000  (  VEE)  -10.0000  ( VOUT)    0.0000  (N06105)    1.7098     

(N06137)    0.0000 (N06291)     .0049 (N06872)    9.8620 




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_V4         0.000E+00
    V_V3         0.000E+00
    V_V2        -6.167E-05

    TOTAL POWER DISSIPATION   6.17E-04  WATTS



          JOB CONCLUDED

**** 02/17/12 14:26:40 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_8\chap8_ex8-9-pspicefiles\schematic1\bias.sim ] 


 ****     JOB STATISTICS SUMMARY


******************************************************************************



  Total job time (using Solver 1)   =         .03
