
**** 02/17/12 13:37:35 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_8\chap8_ex8-6-pspicefiles\schematic1\bias.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "bias.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
* From [PSPICE NETLIST] section of C:\OrCAD\OrCAD_10.5\tools\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.AC DEC 101 1 100k
.PROBE V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\SCHEMATIC1.net" 



**** INCLUDING SCHEMATIC1.net ****
* source CHAP8_EX8-6
R_R22         N01920 VCC  47k  
V_V3         N01952 0 DC 0Vdc AC 1Vac 
V_V2         VCC 0 10v
R_RS         N01952 N02345  0.2k  
C_Cc1         N02345 N01920  2uF  
R_RC         VOUT VCC  2k  
Q_Q22         VOUT N01920 0 Q2N3904
R_R23         0 N01920  3.9k  

**** RESUMING bias.cir ****
.END

**** 02/17/12 13:37:35 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_8\chap8_ex8-6-pspicefiles\schematic1\bias.sim ] 


 ****     BJT MODEL PARAMETERS


******************************************************************************




               Q2N3904         
               NPN             
       LEVEL    1            
          IS    6.734000E-15 
          BF  416.4          
          NF    1            
         VAF   74.03         
         IKF     .06678      
         ISE    6.734000E-15 
          NE    1.259        
          BR     .7371       
          NR    1            
         ISS    0            
          RB   10            
          RE    0            
          RC    1            
         CJE    4.493000E-12 
         VJE     .75         
         MJE     .2593       
         CJC    3.638000E-12 
         VJC     .75         
         MJC     .3085       
        XCJC    1            
         CJS    0            
         VJS     .75         
          TF  301.200000E-12 
         XTF    2            
         VTF    4            
         ITF     .4          
          TR  239.500000E-09 
         XTB    1.5          
          KF    0            
          AF    1            
          CN    2.42         
           D     .87         


**** 02/17/12 13:37:35 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_8\chap8_ex8-6-pspicefiles\schematic1\bias.sim ] 


 ****     SMALL SIGNAL BIAS SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(  VCC)   10.0000  ( VOUT)    3.8079  (N01920)     .6948 (N01952)    0.0000     

(N02345)    0.0000 




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_V3         0.000E+00
    V_V2        -3.294E-03

    TOTAL POWER DISSIPATION   3.29E-02  WATTS



          JOB CONCLUDED

**** 02/17/12 13:37:35 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_8\chap8_ex8-6-pspicefiles\schematic1\bias.sim ] 


 ****     JOB STATISTICS SUMMARY


******************************************************************************



  Total job time (using Solver 1)   =         .06
