("FILE_TYPE"	"PMAP File"
    ("devices"
        ("R"
            ("info"
                ("spice_dsg"	"R")
                ("port_order"
                    ("1")
                    ("2")
                )
            )
            ("model_params"
                ("level_0"
                    ("TC1"
                        ("value"	"0")
                    )
                    ("TC2"
                        ("value"	"0")
                    )
                    ("VALUE"
                        ("value"	"0")
                    )
                )
            )
            ("smoke"
                ("pre_smoke"
                    ("NODE_VA"	"1")
                    ("NODE_VB"	"2")
                    ("DERATE_TYPE"	"RES")
                )
                ("max_ops"
                    ("RV"	"VOLTAGE")
                    ("PDM"	"POWER")
                    ("SLP"	"SLOPE")
                    ("RBA"	"1/SLP")
                    ("TMAX"	"MAX_TEMP")
                    ("TB"	"TMAX")
                )
                ("smoke_tests"
                    ("PDM"
                        ("test"	"power_test")
                    )
                    ("RV"
                        ("test"	"abs_voltage_test")
                        ("nodes"
                            ("NODE_VA")
                            ("NODE_VB")
                        )
                    )
                    ("TB"
                        ("test"	"temp_null_test")
                    )
                )
                ("device_max_ops")
            )
        )
        ("C"
            ("info"
                ("spice_dsg"	"C")
                ("port_order"
                    ("1")
                    ("2")
                )
            )
            ("model_params"
                ("level_0"
                    ("IC"
                        ("value"	"0")
                    )
                    ("TC"
                        ("value"	"0")
                    )
                    ("VALUE"
                        ("value"	"0")
                    )
                )
            )
            ("smoke"
                ("pre_smoke"
                    ("NODE_VA"	"1")
                    ("NODE_VB"	"2")
                    ("TERM_A"	"-1")
                    ("DERATE_TYPE"	"CAP")
                )
                ("max_ops"
                    ("CV"	"VOLTAGE")
                    ("CI"	"CURRENT")
                    ("SLP"	"SLOPE")
                    ("TBRK"	"KNEE")
                    ("TMAX"	"MAX_TEMP")
                )
                ("smoke_tests"
                    ("CV"
                        ("test"	"abs_voltage_test")
                        ("nodes"
                            ("NODE_VA")
                            ("NODE_VB")
                        )
                    )
                    ("CI"
                        ("test"	"abs_current_test")
                        ("term"	"TERM_A")
                    )
                )
                ("device_max_ops")
            )
        )
        ("VDC")
        ("VAC")
        ("Q2N3904"
            ("info"
                ("spice_dsg"	"X")
            )
            ("model_params"
                ("level_0"
                    ("IS"
                        ("value"	"0.1f")
                    )
                    ("BF"
                        ("value"	"100")
                    )
                    ("NF"
                        ("value"	"1")
                    )
                    ("VAF"
                        ("value"	"100MEG")
                    )
                    ("IKF"
                        ("value"	"10")
                    )
                    ("ISE"
                        ("value"	"1E-13")
                    )
                    ("NE"
                        ("value"	"1.5")
                    )
                    ("BR"
                        ("value"	"1")
                    )
                    ("NR"
                        ("value"	"1")
                    )
                    ("VAR"
                        ("value"	"100MEG")
                    )
                    ("IKR"
                        ("value"	"100MEG")
                    )
                    ("ISC"
                        ("value"	"1E-15")
                    )
                    ("NC"
                        ("value"	"2")
                    )
                    ("RB"
                        ("value"	"0")
                    )
                    ("IRB"
                        ("value"	"100MEG")
                    )
                    ("RBM"
                        ("value"	"0")
                    )
                    ("RE"
                        ("value"	"0")
                    )
                    ("RC"
                        ("value"	"0")
                    )
                    ("CJE"
                        ("value"	"0")
                    )
                    ("VJE"
                        ("value"	"0.75")
                    )
                    ("MJE"
                        ("value"	"0.33")
                    )
                    ("TF"
                        ("value"	"0")
                    )
                    ("XTF"
                        ("value"	"0")
                    )
                    ("VTF"
                        ("value"	"100MEG")
                    )
                    ("ITF"
                        ("value"	"0")
                    )
                    ("PTF"
                        ("value"	"0")
                    )
                    ("CJC"
                        ("value"	"0")
                    )
                    ("VJC"
                        ("value"	"0.75")
                    )
                    ("MJC"
                        ("value"	"0.33")
                    )
                    ("XCJC"
                        ("value"	"1")
                    )
                    ("TR"
                        ("value"	"0")
                    )
                    ("CJS"
                        ("value"	"0")
                    )
                    ("VJS"
                        ("value"	"0.75")
                    )
                    ("MJS"
                        ("value"	"0")
                    )
                    ("XTB"
                        ("value"	"0")
                    )
                    ("EG"
                        ("value"	"1.11")
                    )
                    ("XTI"
                        ("value"	"3")
                    )
                    ("KF"
                        ("value"	"0")
                    )
                    ("AF"
                        ("value"	"1")
                    )
                    ("FC"
                        ("value"	"0.5")
                    )
                )
            )
            ("smoke"
                ("max_ops_desc"
                    ("IB"
                        ("description"	"Max base current")
                        ("unit"	"A")
                    )
                    ("IC"
                        ("description"	"Max collector current")
                        ("unit"	"A")
                    )
                    ("VCB"
                        ("description"	"Max C-B voltage")
                        ("unit"	"V")
                    )
                    ("VCE"
                        ("description"	"Max C-E voltage")
                        ("unit"	"V")
                    )
                    ("VEB"
                        ("description"	"Max E-B voltage")
                        ("unit"	"V")
                    )
                    ("PDM"
                        ("description"	"Max pwr dissipation")
                        ("unit"	"W")
                    )
                    ("TJ"
                        ("description"	"Max junction temp")
                        ("unit"	"C")
                    )
                    ("RJC"
                        ("description"	"J-C thermal resist")
                        ("unit"	"C/W")
                    )
                    ("RCA"
                        ("description"	"C-A thermal resist")
                        ("unit"	"C/W")
                    )
                    ("SBSLP"
                        ("description"	"Second brkdown slope")
                        ("unit"	"")
                    )
                    ("SBINT"
                        ("description"	"Sec brkdwn intercept")
                        ("unit"	"A")
                    )
                    ("SBTSLP"
                        ("description"	"SB temp derate slope")
                        ("unit"	"%/C")
                    )
                    ("SBMIN"
                        ("description"	"SB temp derate at TJ")
                        ("unit"	"%")
                    )
                )
                ("pre_smoke"
                    ("TERM_IC"	"-1")
                    ("TERM_IB"	"-2")
                    ("NODE_VC"	"C")
                    ("NODE_VB"	"B")
                    ("NODE_VE"	"E")
                    ("DERATE_TYPE"	"NPN")
                )
                ("max_ops"
                    ("RCA"	"RCA")
                )
                ("smoke_tests"
                    ("IC"
                        ("test"	"current_test")
                        ("term"	"TERM_IC")
                    )
                    ("IB"
                        ("test"	"current_test")
                        ("term"	"TERM_IB")
                    )
                    ("PDM"
                        ("test"	"power_test")
                    )
                    ("SB"
                        ("test"	"breakdown_test")
                        ("term"	"TERM_IC")
                        ("nodes"
                            ("NODE_VC")
                            ("NODE_VE")
                        )
                    )
                    ("TJ"
                        ("test"	"temp_null_test")
                    )
                    ("VCB"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_VC")
                            ("NODE_VB")
                        )
                    )
                    ("VCE"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_VC")
                            ("NODE_VE")
                        )
                    )
                    ("VEB"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_VE")
                            ("NODE_VB")
                        )
                    )
                )
                ("device_max_ops"
                    ("VCB"	"60")
                    ("VCE"	"40")
                    ("VEB"	"6")
                )
                ("device_pre_smoke"
                    ("TERM_IC"	"C")
                    ("TERM_IB"	"B")
                    ("NODE_VC"	"C")
                    ("NODE_VB"	"B")
                    ("NODE_VE"	"E")
                    ("DERATE_TYPE"	"NPN")
                )
            )
        )
    )
    ("instances"
        ("RE"
            ("device_name"	"R")
            ("pspice_path"	"R_RE")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"4.3k")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("Cc2"
            ("device_name"	"C")
            ("pspice_path"	"C_Cc2")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"2uF")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
            )
            ("smoke_vars"
                ("VOLTAGE"	"50.0")
                ("CURRENT"	"1.0")
                ("SLOPE"	"0.005")
                ("KNEE"	"125.0")
                ("MAX_TEMP"	"125.0")
            )
        )
        ("V2"
            ("device_name"	"VDC")
            ("pspice_path"	"V_V2")
            ("level"	"0")
            ("model_params"
                ("DC"
                    ("value"	"10v")
                    ("pspice_param"	"DC")
                )
            )
        )
        ("RS"
            ("device_name"	"R")
            ("pspice_path"	"R_RS")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"0.5k")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("V4"
            ("device_name"	"VDC")
            ("pspice_path"	"V_V4")
            ("level"	"0")
            ("model_params"
                ("DC"
                    ("value"	"10v")
                    ("pspice_param"	"DC")
                )
            )
        )
        ("RL"
            ("device_name"	"R")
            ("pspice_path"	"R_RL")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"3k")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("R2"
            ("device_name"	"R")
            ("pspice_path"	"R_R2")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"100k")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("R1"
            ("device_name"	"R")
            ("pspice_path"	"R_R1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"100k")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("RC"
            ("device_name"	"R")
            ("pspice_path"	"R_RC")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"4.7k")
                    ("pspice_param"	"VALUE")
                )
            )
        )
        ("Cc1"
            ("device_name"	"C")
            ("pspice_path"	"C_Cc1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"2uF")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
            )
            ("smoke_vars"
                ("VOLTAGE"	"50.0")
                ("CURRENT"	"1.0")
                ("SLOPE"	"0.005")
                ("KNEE"	"125.0")
                ("MAX_TEMP"	"125.0")
            )
        )
        ("CE"
            ("device_name"	"C")
            ("pspice_path"	"C_CE")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"150uF")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
            )
            ("smoke_vars"
                ("VOLTAGE"	"50.0")
                ("CURRENT"	"1.0")
                ("SLOPE"	"0.005")
                ("KNEE"	"125.0")
                ("MAX_TEMP"	"125.0")
            )
        )
        ("V3"
            ("device_name"	"VAC")
            ("pspice_path"	"V_V3")
            ("level"	"0")
            ("model_params"
                ("DC"
                    ("value"	"0Vdc")
                    ("pspice_param"	"DC")
                )
                ("ACMAG"
                    ("value"	"1Vac")
                    ("pspice_param"	"AC")
                )
            )
        )
        ("Q22"
            ("device_name"	"Q2N3904")
            ("pspice_path"	"Q_Q22")
            ("level"	"0")
        )
    )
)
