
**** 02/17/12 00:04:22 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Temp\chap10_ex10-9-pspicefiles\schematic1\bias.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "bias.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
* From [PSPICE NETLIST] section of C:\OrCAD\OrCAD_10.5\tools\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.DC LIN vin -8.0v 8.0v 0.01v 
.PROBE V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\SCHEMATIC1.net" 



**** INCLUDING SCHEMATIC1.net ****
* source CHAP10_EX10-9
V_VCC1         0 N25605 10V
R_RL         0 VOUT  6  
Q_Q1         N24710 VIN VOUT Q2N3904
Q_Q3         N25605 VIN VOUT Q2N3906
V_V1         VIN 0  
+SIN 0v 8v 1khz 0 0 0
V_VCC         N24710 0 10V

**** RESUMING bias.cir ****
.END


ERROR -- DC device vin is undefined