
**** 02/16/12 22:30:54 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_5\chap5_ex5-5-pspicefiles\schematic1\bias.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "bias.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
.LIB "../../../chap5_ex5-5-pspiceFiles/cs_with_rs_bias.lib" 
* From [PSPICE NETLIST] section of C:\OrCAD\OrCAD_10.5\tools\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.PROBE V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\SCHEMATIC1.net" 



**** INCLUDING SCHEMATIC1.net ****
* source CH5_EX5-5
R_R1         N23725 N23741  382k  
M_M2         N23773 N23725 N24090 N24090 Mbreakn           
R_R2         N23731 N23725  98k  
R_RD         N23773 N23741  34k  
V_VDD         N23741 0 12V
R_RS         N23731 N24090  4k  
V_-VDD         0 N23731 12V

**** RESUMING bias.cir ****
.END

**** 02/16/12 22:30:54 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_5\chap5_ex5-5-pspicefiles\schematic1\bias.sim ] 


 ****     MOSFET MODEL PARAMETERS


******************************************************************************




               Mbreakn         
               NMOS            
       LEVEL    3            
           L    2.000000E-06 
           W    1.000000E-03 
         VTO    1.5          
          KP    1.035943E-06 
       GAMMA    0            
         PHI     .6          
      LAMBDA    0            
          RD     .01         
          RS     .01         
          RG    5            
          RB    1.000000E-03 
         RDS    1.000000E+06 
          IS   10.000000E-15 
          JS    0            
          PB     .8          
        PBSW     .8          
         CBD    1.000000E-09 
          CJ    0            
        CJSW    0            
        CGSO   40.000000E-12 
        CGDO   10.000000E-12 
        CGBO    0            
         TOX    2.000000E-06 
          XJ    0            
       UCRIT   10.000000E+03 
       KAPPA    1.000000E-12 
      DIOMOD    1            
         VFB    0            
        LETA    0            
        WETA    0            
          U0    0            
        TEMP    0            
         VDD    0            
       XPART    0            


**** 02/16/12 22:30:54 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_5\chap5_ex5-5-pspicefiles\schematic1\bias.sim ] 


 ****     SMALL SIGNAL BIAS SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(N23725)   -7.1000 (N23731)  -12.0000 (N23741)   12.0000 (N23773)   -5.1092     

(N24090)   -9.9872 




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_VDD       -5.532E-04
    V_-VDD      -5.532E-04

    TOTAL POWER DISSIPATION   1.33E-02  WATTS



          JOB CONCLUDED

**** 02/16/12 22:30:54 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_5\chap5_ex5-5-pspicefiles\schematic1\bias.sim ] 


 ****     JOB STATISTICS SUMMARY


******************************************************************************



  Total job time (using Solver 1)   =        0.00
