
**** 02/16/12 23:04:05 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_6\chap6_ex6-4-pspicefiles\schematic1\bias.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "bias.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
.LIB "../../../chap6_ex6-4-pspiceFiles/cd_amp.lib" 
* From [PSPICE NETLIST] section of C:\OrCAD\OrCAD_10.5\tools\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 5ms 0 0.01ms 
.PROBE V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\SCHEMATIC1.net" 



**** INCLUDING SCHEMATIC1.net ****
* source CH6_EX6-4
M_M2         N28161 N28111 VOUT VOUT Mbreakn           
R_RS         0 VOUT  0.5k  
R_RSS         VIN N28287  4k  
R_R1         N28111 N28161  80k  
V_Vin         VIN 0  
+SIN 0 0.5V 1kHz 0 0 0
R_R2         0 N28111  240k  
C_CC         N28287 N28111  100u  
V_VDD         N28161 0 12V

**** RESUMING bias.cir ****
.END

Unable to find index file cd_amp.ind for library file cd_amp.lib
Making new index file cd_amp.ind for library file cd_amp.lib
Index has 1 entries from 1 file(s).

**** 02/16/12 23:04:05 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_6\chap6_ex6-4-pspicefiles\schematic1\bias.sim ] 


 ****     MOSFET MODEL PARAMETERS


******************************************************************************




               Mbreakn         
               NMOS            
       LEVEL    3            
           L    2.000000E-06 
           W     .0154       
         VTO    1.5          
          KP    1.035943E-06 
       GAMMA    0            
         PHI     .6          
      LAMBDA    0            
          RD     .01         
          RS     .01         
          RG    5            
          RB    1.000000E-03 
         RDS    1.000000E+06 
          IS   10.000000E-15 
          JS    0            
          PB     .8          
        PBSW     .8          
         CBD    1.000000E-09 
          CJ    0            
        CJSW    0            
        CGSO   40.000000E-12 
        CGDO   10.000000E-12 
        CGBO    0            
         TOX    2.000000E-06 
          XJ    0            
       UCRIT   10.000000E+03 
       KAPPA    1.000000E-12 
      DIOMOD    1            
         VFB    0            
        LETA    0            
        WETA    0            
          U0    0            
        TEMP    0            
         VDD    0            
       XPART    0            


**** 02/16/12 23:04:05 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_6\chap6_ex6-4-pspicefiles\schematic1\bias.sim ] 


 ****     INITIAL TRANSIENT SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(  VIN)    0.0000  ( VOUT)    5.7956  (N28111)    9.0000 (N28161)   12.0000     

(N28287)    0.0000 




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_Vin        0.000E+00
    V_VDD       -1.163E-02

    TOTAL POWER DISSIPATION   1.40E-01  WATTS



          JOB CONCLUDED

**** 02/16/12 23:04:05 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_6\chap6_ex6-4-pspicefiles\schematic1\bias.sim ] 


 ****     JOB STATISTICS SUMMARY


******************************************************************************



  Total job time (using Solver 1)   =         .05
