
**** 02/16/12 22:14:03 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-dc"  [ D:\AH_kwshin\Lec_Note\cir\Pspice\cs-pspicefiles\schematic1\dc.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "dc.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
.LIB "../../../cs-pspicefiles/cs.lib" 
* From [PSPICE NETLIST] section of C:\OrCAD\OrCAD_10.5\tools\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 5ms 0 0.01ms 
.PROBE V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\SCHEMATIC1.net" 



**** INCLUDING SCHEMATIC1.net ****
* source CS
V_Vin         VIN 0  
+SIN 0 50mV 1kHz 0 0 0
C_CC         N14818 N00145  100u  
R_R1         N00145 N00195  40k  
R_R2         0 N00145  20k  
R_RSS         VIN N14818  1k  
M_M2         VOUT N00145 0 0 Mbreakn  
+ L=2um  
+ W=770u         
R_RD         VOUT N00195  7.5k  
V_VDD         N00195 0 12V

**** RESUMING dc.cir ****
.END

**** 02/16/12 22:14:03 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-dc"  [ D:\AH_kwshin\Lec_Note\cir\Pspice\cs-pspicefiles\schematic1\dc.sim ] 


 ****     MOSFET MODEL PARAMETERS


******************************************************************************




               Mbreakn         
               NMOS            
       LEVEL    3            
           L    2.000000E-06 
           W    1.150000E-03 
         VTO    1.6          
          KP    1.035943E-06 
       GAMMA    0            
         PHI     .6          
      LAMBDA    0            
          RD     .01         
          RS     .01         
          RG    5            
          RB    1.000000E-03 
         RDS    1.000000E+06 
          IS   10.000000E-15 
          JS    0            
          PB     .8          
        PBSW     .8          
         CBD    1.000000E-09 
          CJ    0            
        CJSW    0            
        CGSO   40.000000E-12 
        CGDO   10.000000E-12 
        CGBO    0            
         TOX    2.000000E-06 
          XJ    0            
       UCRIT   10.000000E+03 
       KAPPA    1.000000E-12 
      DIOMOD    1            
         VFB    0            
        LETA    0            
        WETA    0            
          U0    0            
        TEMP    0            
         VDD    0            
       XPART    0            


**** 02/16/12 22:14:03 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-dc"  [ D:\AH_kwshin\Lec_Note\cir\Pspice\cs-pspicefiles\schematic1\dc.sim ] 


 ****     INITIAL TRANSIENT SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(  VIN)    0.0000  ( VOUT)    3.3600  (N00145)    4.0000 (N00195)   12.0000     

(N14818)    0.0000 




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_Vin        0.000E+00
    V_VDD       -1.352E-03

    TOTAL POWER DISSIPATION   1.62E-02  WATTS



          JOB CONCLUDED

**** 02/16/12 22:14:03 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-dc"  [ D:\AH_kwshin\Lec_Note\cir\Pspice\cs-pspicefiles\schematic1\dc.sim ] 


 ****     JOB STATISTICS SUMMARY


******************************************************************************



  Total job time (using Solver 1)   =         .03
