
**** 02/20/12 20:16:40 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_7\chap7_ex7-1-pspicefiles\schematic1\bias.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "bias.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
* From [PSPICE NETLIST] section of C:\OrCAD\OrCAD_10.5\tools\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.DC LIN V_V1 -1v 1v 0.01v 
.PROBE V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\SCHEMATIC1.net" 



**** INCLUDING SCHEMATIC1.net ****
* source CHAP7_EX7-1
V_V1         N21848 0 DC 0.1v  
R_RC2         N21326 N20437  20k  
I_I1         N20419 N21592 DC 250uAdc  
V_VCC1         0 N21592 12V
R_RC1         VOUT N20437  20k  
V_V2         N22086 0 DC 0v  
Q_Q1         VOUT N21848 N20419 Q2N2222
Q_Q2         N21326 N22086 N20419 Q2N2222
V_VCC         N20437 0 12V

**** RESUMING bias.cir ****
.END

**** 02/20/12 20:16:40 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_7\chap7_ex7-1-pspicefiles\schematic1\bias.sim ] 


 ****     BJT MODEL PARAMETERS


******************************************************************************




               Q2N2222         
               NPN             
       LEVEL    1            
          IS   14.340000E-15 
          BF  255.9          
          NF    1            
         VAF   74.03         
         IKF     .2847       
         ISE   14.340000E-15 
          NE    1.307        
          BR    6.092        
          NR    1            
         ISS    0            
          RB   10            
          RE    0            
          RC    1            
         CJE   22.010000E-12 
         VJE     .75         
         MJE     .377        
         CJC    7.306000E-12 
         VJC     .75         
         MJC     .3416       
        XCJC    1            
         CJS    0            
         VJS     .75         
          TF  411.100000E-12 
         XTF    3            
         VTF    1.7          
         ITF     .6          
          TR   46.910000E-09 
         XTB    1.5          
          KF    0            
          AF    1            
          CN    2.42         
           D     .87         



          JOB CONCLUDED

**** 02/20/12 20:16:40 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_7\chap7_ex7-1-pspicefiles\schematic1\bias.sim ] 


 ****     JOB STATISTICS SUMMARY


******************************************************************************



  Total job time (using Solver 1)   =         .03
