
**** 06/02/10 19:53:28 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ C:\AH_kwshin\Lec_Note\cir\Pspice\cs-pspicefiles\schematic1\bias.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "bias.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
.LIB "../../../cs-pspicefiles/cs.lib" 
* From [PSPICE NETLIST] section of C:\OrCAD\OrCAD_10.5\tools\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.OP
.PROBE V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\SCHEMATIC1.net" 



**** INCLUDING SCHEMATIC1.net ****
* source CS
V_Vin         N21673 0  
+SIN 0 50mV 1kHz 0 0 0
C_CC         N14818 N00145  100u  
R_R1         N00145 N00195  50k  
R_R2         0 N00145  20k  
R_RS         N21673 N14818  2k  
M_M2         N00320 N00145 0 0 Mbreakn           
R_RD         N00320 N00195  3k  
V_V1         N00195 0 12

**** RESUMING bias.cir ****
.END

Unable to find index file cs.ind for library file cs.lib
Making new index file cs.ind for library file cs.lib
Index has 1 entries from 1 file(s).

**** 06/02/10 19:53:28 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ C:\AH_kwshin\Lec_Note\cir\Pspice\cs-pspicefiles\schematic1\bias.sim ] 


 ****     MOSFET MODEL PARAMETERS


******************************************************************************




               Mbreakn         
               NMOS            
       LEVEL    3            
           L    2.000000E-06 
           W     .5          
         VTO    1.6          
          KP    1.035943E-06 
       GAMMA    0            
         PHI     .6          
      LAMBDA    0            
          RD     .01         
          RS     .01         
          RG    5            
          RB    1.000000E-03 
         RDS    1.000000E+06 
          IS   10.000000E-15 
          JS    0            
          PB     .8          
        PBSW     .8          
         CBD    1.000000E-09 
          CJ    0            
        CJSW    0            
        CGSO   40.000000E-12 
        CGDO   10.000000E-12 
        CGBO    0            
         TOX    2.000000E-06 
          XJ    0            
       UCRIT   10.000000E+03 
       KAPPA    1.000000E-12 
      DIOMOD    1            
         VFB    0            
        LETA    0            
        WETA    0            
          U0    0            
        TEMP    0            
         VDD    0            
       XPART    0            


**** 06/02/10 19:53:28 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ C:\AH_kwshin\Lec_Note\cir\Pspice\cs-pspicefiles\schematic1\bias.sim ] 


 ****     SMALL SIGNAL BIAS SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(N00145)    3.4286 (N00195)   12.0000 (N00320)     .0085 (N14818)    0.0000     

(N21673)    0.0000 




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_Vin        0.000E+00
    V_V1        -4.169E-03

    TOTAL POWER DISSIPATION   5.00E-02  WATTS


**** 06/02/10 19:53:28 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ C:\AH_kwshin\Lec_Note\cir\Pspice\cs-pspicefiles\schematic1\bias.sim ] 


 ****     OPERATING POINT INFORMATION      TEMPERATURE =   27.000 DEG C


******************************************************************************






**** MOSFETS


NAME         M_M2      
MODEL        Mbreakn   
ID           4.00E-03 
VGS          3.43E+00 
VDS          8.54E-03 
VBS          0.00E+00 
VTH          1.60E+00 
VDSAT        1.83E+00 
Lin0/Sat1   -1.00E+00 
if          -1.00E+00 
ir          -1.00E+00 
TAU         -1.00E+00 
GM           2.19E-03 
GDS          4.71E-01 
GMB          0.00E+00 
CBD          9.95E-10 
CBS          0.00E+00 
CGSOV        2.00E-11 
CGDOV        5.00E-12 
CGBOV        0.00E+00 
CGS          8.63E-12 
CGD          8.63E-12 
CGB          0.00E+00 

          JOB CONCLUDED

**** 06/02/10 19:53:28 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ C:\AH_kwshin\Lec_Note\cir\Pspice\cs-pspicefiles\schematic1\bias.sim ] 


 ****     JOB STATISTICS SUMMARY


******************************************************************************



  Total job time (using Solver 1)   =         .11
