
**** 06/04/10 21:02:14 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ C:\AH_kwshin\Lec_Note\cir\Pspice\cs_cs-pspicefiles\schematic1\bias.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "bias.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
.LIB "../../../cs_cs-pspicefiles/cs_cs.lib" 
* From [PSPICE NETLIST] section of C:\OrCAD\OrCAD_10.5\tools\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 5ms 0 0.01ms 
.PROBE V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\SCHEMATIC1.net" 



**** INCLUDING SCHEMATIC1.net ****
* source CS_CS
R_R2         0 N25325  150k  
R_RD1         VOUT1 N25355  34k  
R_RS2         0 N30302  0  
------------------------$
ERROR -- Value may not be 0
R_R3         VIN N26571  1k  
V_VDD         N25355 0 12V
R_RD2         VOUT N25355  7k  
V_V1         VIN 0  
+SIN 0 50m 1kHz 0 0 0
M_M2         VOUT1 N25325 N25451 N25451 Mbreakn           
R_RS1         0 N25451  0  
------------------------$
ERROR -- Value may not be 0
C_C1         N26571 N25325  100u  
M_M3         VOUT VOUT1 N30302 N30302 Mbreakn           
R_R1         N25325 N25355  450k  

**** RESUMING bias.cir ****
.END
