
**** 02/16/12 22:32:40 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias1"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_5\chap5_ex5-2-pspicefiles\schematic1\bias1.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "bias1.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
.LIB "../../../chap5_ex5-2-pspiceFiles/mos_bias1.lib" 
* From [PSPICE NETLIST] section of C:\OrCAD\OrCAD_10.5\tools\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.PROBE V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\SCHEMATIC1.net" 



**** INCLUDING SCHEMATIC1.net ****
* source CH5_EX5-2
M_M2         N18997 N18927 0 0 Mbreakn           
V_V2         N19089 0 DC 0Vdc AC 1Vac 
R_R1         N18927 N18943  40k  
R_R2         0 N18927  20k  
R_R6         N19089 N19127  1k  
R_RD         N18997 N18943  7.5k  
C_CC         N19127 N18927  100uF  
V_VDD         N18943 0 12V

**** RESUMING bias1.cir ****
.END

WARNING -- Library file "D:\AH_kwshin\Pspice_Electronic Circuit\Chap_5\chap5_ex5-2-pspiceFiles\mos_bias1.lib" has changed since index file mos_bias1.ind was created.
WARNING -- The timestamp changed from Tue Nov 02 11:38:26 2010 to Thu Feb 16 22:32:33 2012.
Making new index file mos_bias1.ind for library file mos_bias1.lib
Index has 1 entries from 1 file(s).

**** 02/16/12 22:32:40 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias1"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_5\chap5_ex5-2-pspicefiles\schematic1\bias1.sim ] 


 ****     MOSFET MODEL PARAMETERS


******************************************************************************




               Mbreakn         
               NMOS            
       LEVEL    3            
           L    2.000000E-06 
           W  770.000000E-06 
         VTO    2            
          KP    1.035943E-06 
       GAMMA    0            
         PHI     .6          
      LAMBDA    0            
          RD     .01         
          RS     .01         
          RG    5            
          RB    1.000000E-03 
         RDS    1.000000E+06 
          IS   10.000000E-15 
          JS    0            
          PB     .8          
        PBSW     .8          
         CBD    1.000000E-09 
          CJ    0            
        CJSW    0            
        CGSO   40.000000E-12 
        CGDO   10.000000E-12 
        CGBO    0            
         TOX    2.000000E-06 
          XJ    0            
       UCRIT   10.000000E+03 
       KAPPA    1.000000E-12 
      DIOMOD    1            
         VFB    0            
        LETA    0            
        WETA    0            
          U0    0            
        TEMP    0            
         VDD    0            
       XPART    0            


**** 02/16/12 22:32:40 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias1"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_5\chap5_ex5-2-pspicefiles\schematic1\bias1.sim ] 


 ****     SMALL SIGNAL BIAS SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(N18927)    4.0000 (N18943)   12.0000 (N18997)    5.9727 (N19089)    0.0000     

(N19127)    0.0000 




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_V2         0.000E+00
    V_VDD       -1.004E-03

    TOTAL POWER DISSIPATION   1.20E-02  WATTS



          JOB CONCLUDED

**** 02/16/12 22:32:40 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias1"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_5\chap5_ex5-2-pspicefiles\schematic1\bias1.sim ] 


 ****     JOB STATISTICS SUMMARY


******************************************************************************



  Total job time (using Solver 1)   =        0.00
