("FILE_TYPE"	"PMAP File"
    ("devices"
        ("uA741"
            ("info"
                ("spice_dsg"	"X")
            )
            ("model_params"
                ("level_1"
                    ("VOS"
                        ("value"	"1e-6")
                    )
                    ("IB"
                        ("value"	"100e-12")
                    )
                    ("IBOS"
                        ("value"	"1e-12")
                    )
                    ("A0"
                        ("value"	"200000")
                    )
                    ("GBW"
                        ("value"	"1e+6")
                    )
                    ("SRP"
                        ("value"	"0.527e+6")
                    )
                    ("SRM"
                        ("value"	"0.527e+6")
                    )
                )
                ("level_2"
                    ("CMRR"
                        ("value"	"100000")
                    )
                    ("P0"
                        ("value"	"0")
                    )
                    ("PD"
                        ("value"	"50e-3")
                    )
                    ("ISCP"
                        ("value"	"25e-3")
                    )
                    ("ISCM"
                        ("value"	"-25e-3")
                    )
                    ("ROUT"
                        ("value"	"75")
                    )
                    ("ROAC"
                        ("value"	"20")
                    )
                    ("VPDIFF"
                        ("value"	"1")
                    )
                    ("VMDIFF"
                        ("value"	"1")
                    )
                    ("VCC"
                        ("value"	"15")
                    )
                    ("VSS"
                        ("value"	"-15")
                    )
                )
                ("level_3"
                    ("CINDM"
                        ("value"	"0")
                    )
                    ("RINDM"
                        ("value"	"10e+9")
                    )
                    ("enw"
                        ("value"	"10e-9")
                    )
                    ("PSRR"
                        ("value"	"1e+5")
                    )
                    ("RLOADP"
                        ("value"	"2000")
                    )
                    ("TCIBOS"
                        ("value"	"0.0")
                    )
                    ("TCIB"
                        ("value"	"0.0")
                    )
                    ("IBT1"
                        ("value"	"0")
                    )
                    ("TMPIB1"
                        ("value"	"0")
                    )
                    ("IBT2"
                        ("value"	"0")
                    )
                    ("TMPIB2"
                        ("value"	"0")
                    )
                    ("TCVOS"
                        ("value"	"0")
                    )
                    ("VOST1"
                        ("value"	"0")
                    )
                    ("TMVOS1"
                        ("value"	"0")
                    )
                    ("VOST2"
                        ("value"	"0")
                    )
                    ("TMVOS2"
                        ("value"	"0")
                    )
                )
            )
            ("smoke"
                ("max_ops_desc"
                    ("IPLUS"
                        ("description"	"Max input current(+)")
                        ("unit"	"A")
                    )
                    ("IMINUS"
                        ("description"	"Max input current(-)")
                        ("unit"	"A")
                    )
                    ("IOUT"
                        ("description"	"Max output current")
                        ("unit"	"A")
                    )
                    ("VDIFF"
                        ("description"	"Max differential VIN")
                        ("unit"	"V")
                    )
                    ("VSMAX"
                        ("description"	"Max supply volt diff")
                        ("unit"	"V")
                    )
                    ("VSMIN"
                        ("description"	"Min supply volt diff")
                        ("unit"	"V")
                    )
                    ("VPMAX"
                        ("description"	"Max inp volt(+)")
                        ("unit"	"V")
                    )
                    ("VPMIN"
                        ("description"	"Min inp volt(+)")
                        ("unit"	"V")
                    )
                    ("VMMAX"
                        ("description"	"Max inp volt(-)")
                        ("unit"	"V")
                    )
                    ("VMMIN"
                        ("description"	"Min inp volt(-)")
                        ("unit"	"V")
                    )
                )
                ("pre_smoke"
                    ("NODE_POS"	"PIN")
                    ("NODE_NEG"	"NIN")
                    ("NODE_VCC"	"PVss")
                    ("NODE_VEE"	"NVss")
                    ("NODE_GND"	"0")
                    ("TERM_POS"	"-1")
                    ("TERM_NEG"	"-2")
                    ("TERM_OUT"	"-3")
                    ("DERATE_TYPE"	"OPAMP")
                )
                ("max_ops")
                ("smoke_tests"
                    ("IMINUS"
                        ("test"	"current_test")
                        ("term"	"TERM_NEG")
                    )
                    ("IPLUS"
                        ("test"	"current_test")
                        ("term"	"TERM_POS")
                    )
                    ("IOUT"
                        ("test"	"abs_current_test")
                        ("term"	"TERM_OUT")
                    )
                    ("VDIFF"
                        ("test"	"abs_voltage_test")
                        ("nodes"
                            ("NODE_POS")
                            ("NODE_NEG")
                        )
                    )
                    ("VMMAX"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_NEG")
                            ("NODE_VCC")
                        )
                    )
                    ("VMMIN"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_VEE")
                            ("NODE_NEG")
                        )
                    )
                    ("VPMAX"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_POS")
                            ("NODE_VCC")
                        )
                    )
                    ("VPMIN"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_VEE")
                            ("NODE_POS")
                        )
                    )
                    ("VSMAX"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_VCC")
                            ("NODE_VEE")
                        )
                    )
                    ("VSMIN"
                        ("test"	"voltage_test")
                        ("nodes"
                            ("NODE_VEE")
                            ("NODE_VCC")
                        )
                    )
                )
                ("device_max_ops"
                    ("VPMIN"	"-7")
                    ("VMMIN"	"-7")
                    ("IOUT"	"40m")
                    ("VDIFF"	"60")
                    ("VSMAX"	"44")
                    ("VSMIN"	"0")
                    ("VPMAX"	"-7")
                    ("VMMAX"	"-7")
                    ("PDM"	"0.5")
                    ("VCCMAX"	"22")
                    ("VEEMAX"	"22")
                )
                ("device_pre_smoke"
                    ("TERM_POS"	"+")
                    ("TERM_NEG"	"-")
                    ("TERM_OUT"	"OUT")
                    ("NODE_POS"	"+")
                    ("NODE_NEG"	"-")
                    ("NODE_GND"	"0")
                    ("NODE_VCC"	"V+")
                    ("NODE_VEE"	"V-")
                    ("DERATE_TYPE"	"OPAMP")
                )
            )
        )
        ("R"
            ("info"
                ("spice_dsg"	"R")
                ("port_order"
                    ("1")
                    ("2")
                )
            )
            ("model_params"
                ("level_0"
                    ("TC1"
                        ("value"	"0")
                    )
                    ("TC2"
                        ("value"	"0")
                    )
                    ("VALUE"
                        ("value"	"0")
                    )
                )
            )
            ("smoke"
                ("pre_smoke"
                    ("NODE_VA"	"1")
                    ("NODE_VB"	"2")
                    ("DERATE_TYPE"	"RES")
                )
                ("max_ops"
                    ("RV"	"VOLTAGE")
                    ("PDM"	"POWER")
                    ("SLP"	"SLOPE")
                    ("RBA"	"1/SLP")
                    ("TMAX"	"MAX_TEMP")
                    ("TB"	"TMAX")
                )
                ("smoke_tests"
                    ("PDM"
                        ("test"	"power_test")
                    )
                    ("RV"
                        ("test"	"abs_voltage_test")
                        ("nodes"
                            ("NODE_VA")
                            ("NODE_VB")
                        )
                    )
                    ("TB"
                        ("test"	"temp_null_test")
                    )
                )
                ("device_max_ops")
            )
        )
        ("VDC")
    )
    ("instances"
        ("U1"
            ("device_name"	"uA741")
            ("pspice_path"	"X_U1")
            ("level"	"0")
        )
        ("R1"
            ("device_name"	"R")
            ("pspice_path"	"R_R1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"2.7k")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
            )
            ("smoke_vars"
                ("POWER"	"0.25")
                ("SLOPE"	"0.005")
                ("MAX_TEMP"	"200.0")
            )
        )
        ("R2"
            ("device_name"	"R")
            ("pspice_path"	"R_R2")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"47k")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
            )
            ("smoke_vars"
                ("POWER"	"0.25")
                ("SLOPE"	"0.005")
                ("MAX_TEMP"	"200.0")
            )
        )
        ("V2"
            ("device_name"	"VDC")
            ("pspice_path"	"V_V2")
            ("level"	"0")
            ("model_params"
                ("DC"
                    ("value"	"12V")
                    ("pspice_param"	"DC")
                )
            )
        )
        ("V1"
            ("device_name"	"VDC")
            ("pspice_path"	"V_V1")
            ("level"	"0")
            ("model_params"
                ("DC"
                    ("value"	"12V")
                    ("pspice_param"	"DC")
                )
            )
        )
    )
)
