
**** 02/16/12 21:09:35 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_2\chap2_design-2-pspicefiles\schematic1\bias.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "bias.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
* From [PSPICE NETLIST] section of C:\OrCAD\OrCAD_10.5\tools\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 3ms 0 1us 
.PROBE V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\SCHEMATIC1.net" 



**** INCLUDING SCHEMATIC1.net ****
* source CH2_DESIGN-2
R_R1         N00214 VOUT  1k  
D_D1         N00254 VOUT D1N4148 
D_D2         VOUT N00268 D1N4148 
V_VS         N00214 0  
+SIN 0 12v 2k 0 0 0
V_V1         0 N00254 4.5Vdc
V_V2         N00268 0 4.5Vdc
R_RL         0 VOUT  3.5k  

**** RESUMING bias.cir ****
.END

**** 02/16/12 21:09:35 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_2\chap2_design-2-pspicefiles\schematic1\bias.sim ] 


 ****     Diode MODEL PARAMETERS


******************************************************************************




               D1N4148         
          IS    2.682000E-09 
           N    1.836        
         ISR    1.565000E-09 
         IKF     .04417      
          BV  100            
         IBV  100.000000E-06 
          RS     .5664       
          TT   11.540000E-09 
         CJO    4.000000E-12 
          VJ     .5          
           M     .3333       


**** 02/16/12 21:09:35 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_2\chap2_design-2-pspicefiles\schematic1\bias.sim ] 


 ****     INITIAL TRANSIENT SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


( VOUT)-1.152E-21  (N00214)    0.0000 (N00254)   -4.5000 (N00268)    4.5000 




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_VS        -1.152E-24
    V_V1        -6.053E-09
    V_V2        -6.053E-09

    TOTAL POWER DISSIPATION   5.45E-08  WATTS



          JOB CONCLUDED

**** 02/16/12 21:09:35 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_2\chap2_design-2-pspicefiles\schematic1\bias.sim ] 


 ****     JOB STATISTICS SUMMARY


******************************************************************************



  Total job time (using Solver 1)   =         .14
