("FILE_TYPE"	"PMAP File"
    ("devices"
        ("R"
            ("info"
                ("spice_dsg"	"R")
                ("port_order"
                    ("1")
                    ("2")
                )
            )
            ("model_params"
                ("level_0"
                    ("TC1"
                        ("value"	"0")
                    )
                    ("TC2"
                        ("value"	"0")
                    )
                    ("VALUE"
                        ("value"	"0")
                    )
                )
            )
            ("smoke"
                ("pre_smoke"
                    ("NODE_VA"	"1")
                    ("NODE_VB"	"2")
                    ("DERATE_TYPE"	"RES")
                )
                ("max_ops"
                    ("RV"	"VOLTAGE")
                    ("PDM"	"POWER")
                    ("SLP"	"SLOPE")
                    ("RBA"	"1/SLP")
                    ("TMAX"	"MAX_TEMP")
                    ("TB"	"TMAX")
                )
                ("smoke_tests"
                    ("PDM"
                        ("test"	"power_test")
                    )
                    ("RV"
                        ("test"	"abs_voltage_test")
                        ("nodes"
                            ("NODE_VA")
                            ("NODE_VB")
                        )
                    )
                    ("TB"
                        ("test"	"temp_null_test")
                    )
                )
                ("device_max_ops")
            )
        )
        ("D1N750"
            ("info"
                ("spice_dsg"	"X")
            )
            ("model_params"
                ("level_0"
                    ("VZT"
                        ("value"	"6.80")
                    )
                    ("IZT"
                        ("value"	"18.5e-03")
                    )
                    ("ZZT"
                        ("value"	"3.6")
                    )
                    ("TCBV"
                        ("value"	"0")
                    )
                    ("IR"
                        ("value"	"0")
                    )
                    ("VR"
                        ("value"	"0")
                    )
                    ("IRM"
                        ("value"	"0")
                    )
                    ("TMAX"
                        ("value"	"150")
                    )
                    ("CJOF"
                        ("value"	"0")
                    )
                    ("VJF"
                        ("value"	"1.0")
                    )
                    ("MF"
                        ("value"	"0.5")
                    )
                    ("ISF"
                        ("value"	"1.345e-14")
                    )
                    ("NF"
                        ("value"	"931.8e-03")
                    )
                    ("RSF"
                        ("value"	"1.074")
                    )
                )
            )
            ("smoke"
                ("max_ops_desc"
                    ("IF"
                        ("description"	"Max Forward Current")
                        ("unit"	"A")
                    )
                    ("IRMX"
                        ("description"	"Max Reverse Current")
                        ("unit"	"A")
                    )
                    ("PDM"
                        ("description"	"Max Pwr Dissipation")
                        ("unit"	"W")
                    )
                    ("TJ"
                        ("description"	"Max Junction Temp")
                        ("unit"	"C")
                    )
                    ("RJC"
                        ("description"	"J-C Thermal Resist")
                        ("unit"	"C/W")
                    )
                    ("RCA"
                        ("description"	"C-A Thermal Resist")
                        ("unit"	"C/W")
                    )
                    ("IMAX"
                        ("description"	"Max. Current A")
                        ("unit"	"")
                    )
                    ("MINR"
                        ("description"	"Min. Resistance Ohm")
                        ("unit"	"")
                    )
                )
                ("pre_smoke"
                    ("TERM_AN"	"-1")
                    ("NODE_AN"	"AN")
                    ("NODE_CAT"	"CAT")
                    ("DERATE_TYPE"	"DIODE")
                )
                ("max_ops"
                    ("RCA"	"RCA")
                )
                ("smoke_tests"
                    ("IF"
                        ("test"	"current_test")
                        ("term"	"TERM_AN")
                    )
                    ("IRMX"
                        ("test"	"neg_current_test")
                        ("term"	"TERM_AN")
                    )
                    ("PDM"
                        ("test"	"power_test")
                    )
                    ("TJ"
                        ("test"	"temp_null_test")
                    )
                )
                ("device_max_ops"
                    ("IF"	"200m")
                    ("IRMX"	"96.72m")
                    ("PDM"	"0.5")
                    ("TJ"	"200")
                    ("RJA"	"300")
                )
                ("device_pre_smoke"
                    ("TERM_AN"	"1")
                    ("NODE_AN"	"1")
                    ("NODE_CAT"	"2")
                    ("DERATE_TYPE"	"DIODE")
                )
            )
        )
    )
    ("instances"
        ("R1"
            ("device_name"	"R")
            ("pspice_path"	"R_R1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"150")
                    ("pspice_param"	"VALUE")
                    ("distrib"	"FLAT")
                )
            )
            ("smoke_vars"
                ("POWER"	"0.25")
                ("SLOPE"	"0.005")
                ("MAX_TEMP"	"200.0")
            )
        )
        ("D1"
            ("device_name"	"D1N750")
            ("pspice_path"	"D_D1")
            ("level"	"0")
        )
    )
)
