
**** 02/17/12 13:26:49 ******* PSpice 10.5.0 (Jan 2005) ******* ID# 2090074177 
 ** Profile: "SCHEMATIC1-bias"  [ D:\AH_kwshin\Pspice_Electronic Circuit\Chap_11\chap11_ex11-17-pspicefiles\schematic1\bias.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "bias.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
* From [PSPICE NETLIST] section of C:\OrCAD\OrCAD_10.5\tools\PSpice\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 300us 0 1us 
.PROBE V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\SCHEMATIC1.net" 



**** INCLUDING SCHEMATIC1.net ****
* source CHAP11_EX11-17
V_V3         VIN 0  
+SIN ov 1.5v 10kHz 0 0 0
-----$
ERROR -- Missing value
R_R1         0 N16676  10k  
R_RF         N16676 VOUT  50k  
X_U1         VIN N16676 VCC VEE VOUT uA741
V_V2         0 VEE 12V
V_V1         VCC 0 12V

**** RESUMING bias.cir ****
.END
